*HEADING
 : F2D2 FLUID ELEMENT TEST
 (1x1x1 BLOCK, HYDRAULIC, NO BULK MODULUS, NO THERMAL EXPANSION)
 KEYWORD-PARAMETER COMBINATION TESTED: CONTROLS, FIELD=HYDROSTATIC FLUID
 PRESSURE
*RESTART, WRITE, FREQ=1
*NODE, NSET=CAV1NOD
*NODE, NSET=CAV2NOD
*ELEMENT, TYPE=F2D2, ELSET=CAV1
*ELEMENT, TYPE=F2D2, ELSET=CAV2
*FLUID PROPERTY, ELSET=CAV1, REFNODE=1, TYPE=HYDRAULIC
*FLUID DENSITY
10.,
*FLUID PROPERTY, ELSET=CAV2, REFNODE=10, TYPE=HYDRAULIC
*FLUID DENSITY
10.,
*ELEMENT, TYPE=SPRING1, ELSET=SPRINGX1
*SPRING, ELSET=SPRINGX1
1,
400.,
*ELEMENT, TYPE=SPRING1, ELSET=SPRINGY1
*SPRING, ELSET=SPRINGY1
2,
1.E-6,
*BOUNDARY
2, 2, 2, 0.0
4, 1, 1, 0.0
20, 2, 2, 0.0
40, 1, 1, 0.0
*EQUATION
**
** Sets added by addodb
**
*Elset,Elset=ODB_ESET
SPRINGX1, SPRINGY1
**
**
*Nset, Nset=ODB_NSET
CAV1NOD,CAV2NOD
**
**  STEP #1: F2D2 FLUID ELEMENT TEST
**
*STEP, NLGEOM
*STATIC
.2, 1.
*CLOAD
4, 2, -600.
*NODE PRINT,FREQ=100,NSET=CAV1NOD
U,PCAV,CVOL
*NODE FILE,FREQ=100,NSET=CAV1NOD
U,PCAV,CVOL
*ENERGY FILE
*ENERGY PRINT
*OUTPUT,FIELD,VARIABLE=PRESELECT,OP=ADD,FREQUENCY=1
*OUTPUT,FIELD, OP=ADD,Frequency=100
*NODE OUTPUT
U,PCAV,CVOL
*OUTPUT,HISTORY,OP=ADD,Frequency=100
*NODE OUTPUT, Nset=ODB_NSET
U,PCAV,CVOL
*OUTPUT,FIELD, OP=ADD
*ENERGY OUTPUT,VARIABLE=ALL
*OUTPUT,HISTORY,OP=ADD
*ENERGY OUTPUT,VARIABLE=ALL
*END STEP
**
** STEP #2, TEST: OPTION *CONTROLS, FIELD=HYDROSTATIC FLUID PRESSURE
**
*STEP, NLGEOM
*STATIC
.2, 1.
*CONTROLS, FIELD=HYDROSTATIC FLUID PRESSURE, PARAMETERS=FIELD
2.5E-3,5.0E-5,3.0E-3,1.0E-2
*CLOAD
40, 2, -600.
*NODE PRINT,FREQ=100,NSET=CAV2NOD
U,PCAV,CVOL
*NODE FILE,FREQ=100,NSET=CAV2NOD
U,PCAV,CVOL
*ENERGY FILE
*ENERGY PRINT
*END STEP