*HEADING
 : FAX2 FLUID ELEMENT TEST
(CYLINDER, R=1 H=1, HYDRAULIC, NO BULK MODULUS, NO THERMAL EXPANSION)
*RESTART, WRITE, FREQ=1
*NODE, NSET=CAV1NOD
*ELEMENT, TYPE=FAX2, ELSET=CAV1
*FLUID PROPERTY, ELSET=CAV1, REFNODE=1, TYPE=HYDRAULIC
*FLUID DENSITY
10.,
*ELEMENT, TYPE=SPRING1, ELSET=SPRINGR1
*SPRING, ELSET=SPRINGR1
1,
400.,
*ELEMENT, TYPE=SPRING1, ELSET=SPRINGZ1
*SPRING, ELSET=SPRINGZ1
2,
1.E-6,
*BOUNDARY
2, 2, 2, 0.0
4, 1, 1, 0.0
*EQUATION
*STEP, NLGEOM
*STATIC
.2, 1.0
*CLOAD
4, 2, -600.
*NODE PRINT,FREQ=100
U,PCAV,CVOL
RF,
*NODE FILE,FREQ=100
U,PCAV,CVOL
RF,
*OUTPUT,FIELD,FREQ=100
*NODE OUTPUT
U,PCAV,CVOL
RF,
*ENERGY FILE
*OUTPUT,HISTORY,FREQUENCY=1
*ENERGY OUTPUT,VARIABLE=PRESELECT
*ENERGY PRINT
*END STEP