*HEADING
 EFA2SXSO: FAX2 FLUID ELEMENT TEST
(CYLINDER, R=1 H=1, HYDRAULIC, NO BULK MODULUS, NO THERMAL EXPANSION)
(TEST FOR CALCUALTION OF REACTIONS)
*RESTART, WRITE, FREQ=1
*NODE, NSET=CAV1NOD
*ELEMENT, TYPE=FAX2, ELSET=CAV1
*FLUID PROPERTY, ELSET=CAV1, REFNODE=1, TYPE=HYDRAULIC
*FLUID DENSITY
10.,
*BOUNDARY
2, 1, 2
3, 1, 2
4, 1, 2
*STEP, NLGEOM
*STATIC
*BOUNDARY
 1,8,8,1.0
*NODE PRINT,FREQ=100, SUMMARY=NO
PCAV,CVOL
RF,
*NODE FILE,FREQ=100
PCAV,CVOL
RF,
*OUTPUT,FIELD,FREQ=100
*NODE OUTPUT
PCAV,CVOL
RF,
*END STEP