*HEADING
: FLEXIBLE JOINT WITH LINEAR BEHAVIOR, DASHPOT SUBOPTION  [JOINTC]
** Same as EXJOXDX1 but with temp/fv dependent spring/dashpot properties
*NODE,NSET=FILE
*ELEMENT,TYPE=DASHPOT1,ELSET=D
*DASHPOT,ELSET=D,NONLINEAR,DEPENDENCIES=2
 1,
 -1.0e-10,-100.00,  0.,0.,0.
  1.0e-10, 100.00,  0.,0.,0.
  -18.000,-100.00,200.,0.,0.
   18.000, 100.00,200.,0.,0.
 -1.0e-10,-100.00,  0.,2.,0.
  1.0e-10, 100.00,  0.,2.,0.
  -22.000,-100.00,200.,2.,0.
*ELEMENT,TYPE=SPRING1,ELSET=S
*SPRING,ELSET=S,DEPENDENCIES=2
 1,
 1.0E-10,,0.,0.,0.
 30.,,  200.,0.,0.
 1.0E-10,,0.,2.,0.
 50.,,  200.,2.,0.
 1.0E-10,,0.,0.,2.
 70.,,  200.,0.,2.
 1.0E-10,,0.,2.,2.
*ELEMENT,TYPE=MASS,ELSET=M
*MASS  ,ELSET=M
0.02588,
**
** JOINTC ELEMENT ADDED
**
*NODE
*NODE,NSET=FILE
*ELEMENT,TYPE=JOINTC,ELSET=JOINT
*JOINT,ELSET=JOINT
*SPRING, DEPENDENCIES=2
 1,
 1.0E-10,,0.,0.,0.
 30.,,  200.,0.,0.
 1.0E-10,,0.,2.,0.
 50.,,  200.,2.,0.
 1.0E-10,,0.,0.,2.
 70.,,  200.,0.,2.
 1.0E-10,,0.,2.,2.
*DASHPOT,NONLINEAR,DEPENDENCIES=2
 1,
 -1.0e-10,-100.00,  0.,0.,0.
  1.0e-10, 100.00,  0.,0.,0.
  -18.000,-100.00,200.,0.,0.
   18.000, 100.00,200.,0.,0.
 -1.0e-10,-100.00,  0.,2.,0.
  1.0e-10, 100.00,  0.,2.,0.
  -22.000,-100.00,200.,2.,0.
*ELEMENT,TYPE=MASS,ELSET=M
*RESTART,WRITE,FREQUENCY=5
*NSET,NSET=NALL
*INITIAL CONDITIONS,TYPE=TEMPERATURE
NALL,0.
*INITIAL CONDITIONS,TYPE=FIELD,VARIABLE=1
NALL,0.
*INITIAL CONDITIONS,TYPE=FIELD,VARIABLE=2
NALL,0.
*AMPLITUDE,NAME=STEPPED
0.,1.,1.E10, 1.
*STEP
  STRETCH OUT
*STATIC
1.E10,1.E10
*BOUNDARY
 1,1,1,1.
100,1,6
101,1,1,1.
101,2,6
*TEMPERATURE,AMPLITUDE=STEPPED
NALL,100.
*FIELD,AMPLITUDE=STEPPED,VARIABLE=1
NALL,1.
*FIELD,AMPLITUDE=STEPPED,VARIABLE=2
NALL,1.
*ENERGY PRINT,FREQ=2
*EL PRINT,FREQ=2,SUMMARY=NO
S,
E,
*NODE PRINT,FREQ=2,SUMMARY=NO
U,
V,
A,
CF,
RF,
*ENERGY FILE,FREQUENCY=10
*NODE FILE,NSET=FILE,FREQ=10
U , V , A
*EL FILE,FREQUENCY=10
S,E
*CONTROLS,PARAM=TIME INC
4,8,9,16,10,4,12,5,6,3
.25,.5,.75,.85,.25,.25,1.5,.75
.8,1.5,1.25,2.0,1.0,.1,1.0,.95
*END STEP
*STEP,INC=200
  RELEASE INITIALLY STRETCHED SYSTEM
*DYNAMIC,HAFTOL=1.
 5.E-4,.7
*BOUNDARY,OP=NEW
100,1,6
101,2,6
*END STEP