*HEADING
CONNECTOR DAMPING OPTIONS - /STANDARD VERIFICATION, CARTESIAN CONNECTION
**
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
**
***************************************
**SECTION 1: CONN3D2 NODES/ELEMENTS  **
***************************************
**
*NODE,NSET=N51
**
*NODE,NSET=N52
**
*NODE,NSET=N54
**
*NODE,NSET=M51
**
*NODE,NSET=M52
**
*NODE,NSET=M54
**
*NODE, NSET=O51
**
*ELEMENT,TYPE=CONN3D2,ELSET=TEST1
*ELEMENT,TYPE=CONN3D2,ELSET=TEST11
*ELEMENT,TYPE=CONN3D2,ELSET=TEST31
*ELEMENT,TYPE=CONN3D2,ELSET=TEST1I
*ELEMENT,TYPE=CONN3D2,ELSET=TEST11I
*ELEMENT,TYPE=CONN3D2,ELSET=TEST31I
*ELEMENT,TYPE=CONN3D2,ELSET=TEST41
**
*ELEMENT,TYPE=MASS,ELSET=MASS
*MASS,ELSET=MASS
1.E-3
**
***********************************************
**SECTION 2:  CONNECTOR BEHAVIOR DEFINITION  **
***********************************************
**
*******************************************************
** *CONNECTOR DAMPING,COMPONENT=1, DEPENDENCIES=2    **
*******************************************************
**
*CONNECTOR SECTION,ELSET=TEST1,BEHAVIOR=TB1
CARTESIAN,
ORIGLOB,
**
*ORIENTATION,SYS=RECT,NAME=ORIGLOB
**
*CONNECTOR BEHAVIOR,NAME=TB1
*CONNECTOR DAMPING,COMPONENT=1,DEPENDENCIES=2
**
*CONNECTOR SECTION,ELSET=TEST1I,BEHAVIOR=TB1
CARTESIAN,
ORIGLOB,
**
****************************************************************
** *CONNECTOR DAMPING,COMPONENT=1,DEPENDENCIES=1,NONLINEAR    **
****************************************************************
**
*CONNECTOR SECTION,ELSET=TEST11,BEHAVIOR=TB11
CARTESIAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TB11
*CONNECTOR DAMPING,COMPONENT=1,DEPENDENCIES=1,NONLINEAR
** LINEAR FOR CHECK WITH CASE 1 ABOVE WITH T=-10, FV1=1, FV2=0.5
**
**
**
*CONNECTOR SECTION,ELSET=TEST11I,BEHAVIOR=TB11
CARTESIAN,
ORIGLOB,
**
**************************************************
** *CONNECTOR DAMPING,DEPENDENCIES=1    **
**************************************************
**
*CONNECTOR SECTION,ELSET=TEST31,BEHAVIOR=TB31
CARTESIAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TB31
*CONNECTOR DAMPING,DEP=1
** CHECK FOR CASE 1 ABOVE WITH T=-10, FV1=1
**
*CONNECTOR SECTION,ELSET=TEST31I,BEHAVIOR=TB31
CARTESIAN,
ORIGLOB,
**
***********************************************************************
** *CONNECTOR DAMPING,COMPONENT=1,INDEPENDENT COMPONENTS=POSITION,NONLINEAR**
***********************************************************************
**
*CONNECTOR SECTION,ELSET=TEST41,BEHAVIOR=TB41
CARTESIAN,
ORIGLOB,
**
** TEST INDEPENDENT COMPONENTS = POSITION
**
*CONNECTOR BEHAVIOR,NAME=TB41
*CONNECTOR DAMPING, COMP=1,INDEPENDENT COMPONENTS=POSITION,NONLINEAR
**
**
**
****************************************
**SECTION 3: DASHPOT ELEMENT BASELINE **
****************************************
**
*NODE,NSET=NT
**
*ELEMENT,TYPE=DASHPOTA,ELSET=DP
*DASHPOT,ELSET=DP,DEPENDENCIES=2
1500.,,-10.,1.,0.5
 750.,, 40.,1.,0.5
 100.,, 90.,1.,0.5
1750.,,-10.,2.,0.5
1000.,, 40.,2.,0.5
 250.,, 90.,2.,0.5
2500.,,-10.,3.,0.5
1450.,, 40.,3.,0.5
**
**
*****************************************************
**SECTION 4: COMMON OPTIONS AND HISTORY DEFINITION **
*****************************************************
**
*BOUNDARY
FIX,1,6
ACT,2,6
*BOUNDARY
8002,3,6
**
*NSET,NSET=ACT
*NSET,NSET=FIX
*NSET,NSET=NALL3D
*NSET,NSET=NALL3DI
*NSET,NSET=NALL
NALL3D,10001,10002,NALL3DI
**
*ELSET,ELSET=EALL
*AMPLITUDE,NAME=VP
0.,0.,0.01,1.0
*INITIAL CONDITIONS, TYPE=TEMPERATURE
NALL3D, -10.0
*INITIAL CONDITIONS, TYPE=FIELD, VAR=1
NALL3D, 1.0
*INITIAL CONDITIONS, TYPE=FIELD, VAR=2
NALL3D, 0.5
*INITIAL CONDITIONS, TYPE=TEMPERATURE
NALL3DI, 90.0
*INITIAL CONDITIONS, TYPE=FIELD, VAR=1
NALL3DI, 2.0
*INITIAL CONDITIONS, TYPE=FIELD, VAR=2
NALL3DI, 1.0
*INITIAL CONDITIONS, TYPE=VELOCITY
NALL,1,0.0
**
**********************
*STEP,NLGEOM=YES,INC=1100
CONNECTOR DAMPING TEST STEP - PRESCRIBED LOAD
*DYNAMIC,DIRECT
0.0001, 0.01
**
*TEMPERATURE
NALL,-10.
*FIELD,VAR=1
NALL,1.0
*FIELD,VAR=2
NALL,0.5
*TEMPERATURE
NALL3DI,90.
*FIELD,VAR=1
NALL3DI,2.0
*FIELD,VAR=2
NALL3DI,1.0
**
*CLOAD, AMP=VP
5002,1, 15.
5012,1, 15.
5032,1, 15.
10002,1, 15.
7002,1, 15.
7012,1, 15.
7032,1, 15.
8002,1, 15.
**
*CONNECTOR MOTION
**
*OUTPUT,FIELD,FREQ=1
*ELEMENT OUTPUT, ELSET=EALL
NFORC,ELEN
*NODE OUTPUT,VAR=ALL
**
*OUTPUT,HISTORY,FREQ=1
*NODE OUTPUT,NSET=NALL
U,V,A,RF
*ELEMENT OUTPUT,ELSET=EALL
CTF1,CEF1,CRF1,CP1,CU1,CV1,CA1,CVF1,CCF1
*ENDSTEP