*HEADING
CONNECTOR FUNCTIONALITY VERIFICATION - /EXPLICIT,CARTESIAN
**
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
**
**
******************************
**  CONN2D2 NODES/ELEMENTS  **
******************************
**
*NODE,NSET=NALL2D
**
*ELEMENT,TYPE=CONN2D2,ELSET=TESTTF
*ELEMENT,TYPE=CONN2D2,ELSET=TESTTD
**
*ELSET,ELSET=EALL
TESTTF,TESTTD
*ELEMENT,TYPE=MASS,ELSET=MASS
**
*MASS,ELSET=MASS
1.E-4,
**
***********************************************************
** DISPLACEMENT LIMITED CONNECTOR FAILURE FOR CARTESIAN  **
***********************************************************
**
*CONNECTOR SECTION,ELSET=TESTTD,BEHAVIOR=TBTD
CARTESIAN,
ORIGLOB,
**
*ORIENTATION,SYS=RECT,NAME=ORIGLOB
**
*CONNECTOR BEHAVIOR,NAME=TBTD
*CONNECTOR ELASTICITY,COMPONENT=1
*CONNECTOR ELASTICITY,COMPONENT=2
*CONNECTOR FAILURE,COMPONENT=1,RELEASE=ALL
**
*BOUNDARY
11,1,2
11,6,6
**
****************************************************
** FORCE LIMITED CONNECTOR FAILURE FOR CARTESIAN  **
****************************************************
**
*CONNECTOR SECTION,ELSET=TESTTF,BEHAVIOR=TBTF
CARTESIAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBTF
*CONNECTOR ELASTICITY,COMPONENT=1
*CONNECTOR ELASTICITY,COMPONENT=2
*CONNECTOR FAILURE,COMPONENT=1,RELEASE=ALL
**
*BOUNDARY
1,1,2
1,6,6
**
*AMPLITUDE,NAME=VP,DEFINITION=SMOOTH STEP,SMOOTH=0.05
0.,0.,0.01,1.0
**
*NSET,NSET=NALL
NALL2D,
*ELSET,ELSET=TEST
TESTTF,TESTTD
**
*ELSET,ELSET=QA_TEST_EALL
EALL,
*NSET,NSET=QA_TEST_NALL
NALL,
**
*STEP,NLGEOM=NO
CONNECTOR TEST STEP - CONNECTOR FAIL
*DYNAMIC,EXPLICIT,DIRECT USER CONTROL
2.E-4,0.01
**
*BOUNDARY,AMPLITUDE=VP
2,1,2,0.1
12,1,2,0.1
**
*OUTPUT,FIELD,NUMBER INTERVAL=10,TIME MARKS=YES
*ELEMENT OUTPUT,VAR=ALL
*NODE OUTPUT,VAR=ALL
**
*OUTPUT,HISTORY,TIME INTERVAL=2.E-4
*NODE OUTPUT,NSET=NALL
U,V,A,RF
*ELEMENT OUTPUT,ELSET=TEST
CP,CU,CV,CA,CTF,CEF,CRF,CFAILST
ELEN,
**
*FILE OUTPUT,NUMBER INTERVAL=1,TIME MARKS=YES
*NODE FILE,NSET=NALL
U,
*EL FILE,ELSET=EALL
CU,
CP,
CTF,
CEF,
CFAILST
*************************
*OUTPUT, FIELD, NUMBER INTERVAL=1,TIME MARKS=YES
*NODE OUTPUT, NSET=QA_TEST_NALL
U,
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIMEINT=0.01
*************************
***OUTPUT,HISTORY,VARIABLE=PRESELECT
*ENDSTEP