*HEADING
CONNECTOR FUNCTIONALITY VERIFICATION - /STANDARD,CARTESIAN & CARDAN
**
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
**
*NODE,NSET=NALL3D
**
*ELEMENT,TYPE=CONN3D2,ELSET=TESTT
*ELEMENT,TYPE=CONN3D2,ELSET=TESTR
*ELSET, ELSET=TEST
TESTT, TESTR
**
*****************************************
** CONNECTOR ELASTICITY FOR CARTESIAN  **
*****************************************
*CONNECTOR SECTION,ELSET=TESTT,BEHAVIOR=TBT
CARTESIAN,
ORIGLOB,
**
*ORIENTATION,SYS=RECT,NAME=ORIGLOB,DEFINITION=NODES
**
*CONNECTOR BEHAVIOR,NAME=TBT
*CONNECTOR ELASTICITY,COMPONENT=1
**
*BOUNDARY
1001,1,6
1002,2,6
**
***************************************
** CONNECTOR ELASTICITY FOR CARDAN   **
***************************************
**
*CONNECTOR SECTION,ELSET=TESTR,BEHAVIOR=TBR
CARDAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBR
*CONNECTOR ELASTICITY,COMPONENT=4
******************************
**
*BOUNDARY
1011,1,6
1012,1,3
1012,5,6
**
******************************
**
** STEP 1
**
*STEP,NLGEOM=YES,INC=25
CONNECTOR TEST STEP - CONNECTOR MOTION
*STATIC
0.02,1.0
**
*CONNECTOR MOTION,USER
**
*OUTPUT,FIELD,FREQ=1
*ELEMENT OUTPUT,ELSET=TEST
ELEN
*NODE OUTPUT,VAR=ALL
**
*OUTPUT,HISTORY,FREQ=1
*NODE OUTPUT,NSET=NALL3D
U,RF
*ELEMENT OUTPUT,ELSET=TEST
CEF1,CU1,CCF1, CEM1,CRM1, CCM1,CP1, CPR1, CUR1,
CCU1, CCUR1,CRF1, CTF1, CTM1
*ENDSTEP
**
** STEP 2
**
*STEP,NLGEOM=YES,INC=25
CONNECTOR TEST STEP - CONNECTOR MOTION,FIXED
*STATIC
0.02,1.0
**
*CONNECTOR MOTION,FIXED
*CLOAD
1001,1,-350.
1011,4,-350.
**
*ENDSTEP
**
** STEP 3
**
*STEP,NLGEOM=NO,PERT
CONNECTOR TEST STEP - CONNECTOR MOTION, LINEAR PERTURBATION
*STATIC
**
*CONNECTOR MOTION
*OUTPUT,HISTORY,FREQ=1
*NODE OUTPUT,NSET=NALL3D
U,RF
*ELEMENT OUTPUT,ELSET=TEST
CEF1,CU1,CCF1, CEM1,CRM1, CCM1,CP1, CPR1, CUR1,
CCU1, CCUR1,CRF1, CTF1, CTM1
**
*ENDSTEP