*HEADING
TEST DAMAGE INITIATION CONNECTOR AND CONNECTOR DAMAGE EVOLUTION BEHAVIORS - 2D - NON LINEAR ELASTICITY
**PREPRINT, MODEL=YES
**
********************************************************************
**	SECTION I: MODEL DATA
********************************************************************
**
********************** TEST 12 ****************************
*NODE
*ELEMENT, TYPE=CONN2D2, ELSET=C12
*CONNECTOR SECTION, ELSET=C12, BEHAVIOR=B12
CARTESIAN
GLOB12,
*ORIENTATION, NAME=GLOB12
**
*CONNECTOR BEHAVIOR, NAME=B12
*INCLUDE, INPUT=misc_nonlinearelas_dam_conn2d.inp
*INCLUDE, INPUT=misc_dam_mot_lin_2d.inp
**
*ELEMENT, TYPE=MASS, ELSET=M12
*MASS, ELSET=M12
1E-3
*ELEMENT, TYPE=ROTARYI, ELSET=R12
*ROTARY INERTIA, ELSET=R12
1E-4, 1E-4, 1E-4
**
********************** TEST 22 ****************************
*NODE
*ELEMENT, TYPE=CONN2D2, ELSET=C22
*CONNECTOR SECTION, ELSET=C22, BEHAVIOR=B22
CARTESIAN
GLOB22,
*ORIENTATION, NAME=GLOB22
**
*CONNECTOR BEHAVIOR, NAME=B22
*INCLUDE, INPUT=misc_nonlinearelas_dam_conn2d.inp
*INCLUDE, INPUT=misc_dam_mot_exp_2d.inp
**
*ELEMENT, TYPE=MASS, ELSET=M22
*MASS, ELSET=M22
1E-3
*ELEMENT, TYPE=ROTARYI, ELSET=R22
*ROTARY INERTIA, ELSET=R22
1E-4, 1E-4, 1E-4
**
********************** TEST 32 ****************************
*NODE
*ELEMENT, TYPE=CONN2D2, ELSET=C32
*CONNECTOR SECTION, ELSET=C32, BEHAVIOR=B32
CARTESIAN
GLOB32,
*ORIENTATION, NAME=GLOB32
**
*CONNECTOR BEHAVIOR, NAME=B32
*INCLUDE, INPUT=misc_nonlinearelas_dam_conn2d.inp
*INCLUDE, INPUT=misc_dam_mot_tab_2d.inp
**
*ELEMENT, TYPE=MASS, ELSET=M32
*MASS, ELSET=M32
1E-3
*ELEMENT, TYPE=ROTARYI, ELSET=R32
*ROTARY INERTIA, ELSET=R32
1E-4, 1E-4, 1E-4
**
********************** TEST 42 ****************************
*NODE
*ELEMENT, TYPE=CONN2D2, ELSET=C42
*CONNECTOR SECTION, ELSET=C42, BEHAVIOR=B42
CARTESIAN
GLOB42,
*ORIENTATION, NAME=GLOB42
**
*CONNECTOR BEHAVIOR, NAME=B42
*INCLUDE, INPUT=misc_nonlinearelas_dam_conn2d.inp
*INCLUDE, INPUT=misc_dam_mot_ener_2d.inp
**
*ELEMENT, TYPE=MASS, ELSET=M42
*MASS, ELSET=M42
1E-3
*ELEMENT, TYPE=ROTARYI, ELSET=R42
*ROTARY INERTIA, ELSET=R42
1E-4, 1E-4, 1E-4
**
********************************************************************
**	SECTION II: HISTORY DATA
********************************************************************
**
*STEP, NLGEOM=YES
*DYNAMIC, EXPLICIT, DIRECT
1e-4, 1
********************** TEST 12 *************************************
*AMPLITUDE, NAME=CYCLE_12
0.0,0.0,0.25,0.75,0.5,0,1,1.00
*BOUNDARY
121,1,6,
*BOUNDARY, AMPLITUDE=CYCLE_12
122,1,1,1
122,2,2,1
122,3,3,1
122,4,4,1
122,5,5,1
122,6,6,1
*OUTPUT, HISTORY
*ELEMENT OUTPUT, ELSET=C12
CU, CUE, CUP, CUPEQ, CEF, CRF, CDIF, CDIM, CDIP, CDMG
********************** TEST 22 *************************************
*AMPLITUDE, NAME=CYCLE_22
0.0,0.0,0.25,0.75,0.5,0,1,1.00
*BOUNDARY
221,1,6,
*BOUNDARY, AMPLITUDE=CYCLE_22
222,1,1,1
222,2,2,1
222,3,3,1
222,4,4,1
222,5,5,1
222,6,6,1
*OUTPUT, HISTORY
*ELEMENT OUTPUT, ELSET=C22
CU, CUE, CUP, CUPEQ, CEF, CRF, CDIF, CDIM, CDIP, CDMG
********************** TEST 32 *************************************
*AMPLITUDE, NAME=CYCLE_32
0.0,0.0,0.25,0.75,0.5,0,1,1.00
*BOUNDARY
321,1,6,
*BOUNDARY, AMPLITUDE=CYCLE_32
322,1,1,1
322,2,2,1
322,3,3,1
322,4,4,1
322,5,5,1
322,6,6,1
*OUTPUT, HISTORY
*ELEMENT OUTPUT, ELSET=C32
CU, CUE, CUP, CUPEQ, CEF, CRF, CDIF, CDIM, CDIP, CDMG
********************** TEST 42 *************************************
*AMPLITUDE, NAME=CYCLE_42
0.0,0.0,0.25,0.75,0.5,0,1,1.00
*BOUNDARY
421,1,6,
*BOUNDARY, AMPLITUDE=CYCLE_42
422,1,1,1
422,2,2,1
422,3,3,1
422,4,4,1
422,5,5,1
422,6,6,1
*OUTPUT, HISTORY
*ELEMENT OUTPUT, ELSET=C42
CU, CUE, CUP, CUPEQ, CEF, CRF, CDIF, CDIM, CDIP, CDMG
********************************************************************
*END STEP