** : symmetric transfer from base problem: psa2sslin0
** : base problem for symmetric transfer problem: psf4sslin2
*HEADING
 FEATURE TESTED : SYMMETRIC MODEL GENERATION
                  SYMMETRIC RESULTS TRANSFER
 ELEMENT TESTED : SAX1 --> S4R
*SYMMETRIC MODEL GENERATION,REVOLVE,ELEMENT=1000,NODE=1000
*SYMMETRIC RESULTS TRANSFER
*ELSET,ELSET=sect,gen
*nset,nset=sect,gen
*TRANSFORM,NSET=NALL,TYPE=C
*RESTART,WRITE,FREQ=1
*BOUNDARY
 BOT, 1,6
 TOP, 3
 TOP, 5
*STEP,INC=100,NLGEOM
*STATIC,DIRECT
 1.0,1.0
*DLOAD
 ELOAD, P, -10.0
*NODE PRINT,nset=sect
 U,
*EL PRINT,elset=sect
 S,
 SF
*EL PRINT,elset=sect,rebar
 S,
*NODE FILE, F=4
 U,
*EL FILE,ELSET=SECT,F=4
 S,
*ELFILE, ELSET=SECT, F=4, REBAR
 S ,
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=SECT
 S
 SF
*NODE OUTPUT, NSET=SECT
 U
*FILE FORMAT, ZEROINC
*END STEP