** : symmetric transfer from base problem: psf4sslin1
*HEADING
 FEATURE TESTED : SYMMETRIC MODEL GENERATION
                  SYMMETRIC RESULTS TRANSFER
 ELEMENT TESTED : SAX1 --> S4R
*symmetric model generation,reflect=line,tol=0.001,ELEMENT=100000,NODE=100000
*symmetric results transfer
*ELSET,ELSET=sect2
*NSET,NSET=sect2
*TRANSFORM,NSET=NALL,TYPE=C
*RESTART,WRITE,FREQ=1
*BOUNDARY
 BOT, 1,6
*STEP,INC=100,NLGEOM
*STATIC
 1.0,1.0
*DLOAD
 ELOAD, P, -10.0
*NODE PRINT,nset=sect2
 U,
*EL PRINT,elset=sect2
 S,
 SF,
*EL PRINT,elset=sect2,rebar
 S,
*NODE FILE, F=4
 U,
*EL FILE,ELSET=SECT,F=4
 S,
 SF,
*ELFILE, ELSET=SECT, F=4, REBAR
 S ,
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=SECT2
 S,
 SF,
*NODE OUTPUT, NSET=SECT2
 U
*FILE FORMAT, ZEROINC
*END STEP