*HEADING
 STRAIGHT LINE ROLLING INERTIA.
 CCL12H ELEMENTS;  USES 2D DEPENDENCY FILE  pstca4shhia.res
*RESTART,WRITE,FREQ=100
*SYMMETRIC MODEL GENERATION,REVOLVE,NODEOFF=1000,ELEMENT=1000,TRANSPORT
 360.0, 12,,C
*NSET,NSET=SECTR,GEN
*NSET,NSET=SECTS,GEN
*NSET,NSET=SECT
 SECTR, SECTS
*ELSET,ELSET=SECTR,GEN
*ELSET,ELSET=SECTS,GEN
*ELSET,ELSET=SECT
 SECTR, SECTS
*****************************
*STEP,INC=100,NLGEOM
 PLANE STRAIN BOUNDARY CONDITIONS
*STEADY STATE TRANSPORT,INERTIA=YES
*BOUNDARY
 NSIDE, 3
 NRIM,  1, 3
*DLOAD
 ETIRER, CENT, 57.6,   0.0, 0.0, 0.0,  0.0, 0.0, 1.0
*TRANSPORT VELOCITY
 NTIRES, 40.0
*NODE PRINT,NSET=SECTR
 U,
*NODE PRINT,NSET=SECTS
 U,
*EL PRINT,ELSET=SECTR
 S,
*EL PRINT,ELSET=SECTS
 S,
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=SECT
 S
*NODE OUTPUT,NSET=SECT
 U
*OUTPUT,HIST
*END STEP
*****************************
*STEP,INC=100,NLGEOM
 FREE AXIAL DIRECTION
*STEADY STATE TRANSPORT,INERTIA=YES
*BOUNDARY,OP=NEW
 NRIM,  1, 3
*DLOAD
 ETIRER, CENT, 57.6,   0.0, 0.0, 0.0,  0.0, 0.0, 1.0
*TRANSPORT VELOCITY
 NTIRES, 40.0
*END STEP