*HEADING
 Transfer from Standard to Standard : Test for C3D10M element
 - loading in shear
 - with orientation
*IMPORT,STEP=1,UPDATE=NO,STATE=YES
 SHELL,
*IMPORT NSET
 ALL,
*RESTART, WRITE, FREQ=100
**
*FILE FORMAT, ZERO INCREMENT
*BOUNDARY
 1, 1,3
 2, 1,3
 5, 1,2
 6, 1,2
 9, 1,3
13, 1,2
17, 1,2
18, 1,2
*STEP,NLGEOM,INC=50
*STATIC
 0.1, 1.
*BOUNDARY
 3, 1, 1, 0.3
 4, 1, 1, 0.3
 7, 1, 1, 0.3
 8, 1, 1, 0.3
*EL FILE, DIRECTIONS=YES
 S,LE
*NODE FILE
 U,
*EL PRINT, FREQ=100
 S,
 E,
 PEEQ,
*NODE PRINT, FREQ=100
 U,
 COORD,
 RF,
*OUTPUT,HISTORY,VARIABLE=PRESELECT
*OUTPUT,FIELD
*NODE OUTPUT
 U,COORD
*ELEMENT OUTPUT
S,LE,PE,PEEQ
*END STEP