*HEADING
*PREPRINT,MODEL=YES, ECHO=YES, HISTORY=YES
*IMPORT, UPDATE=NO,STATE=YES, STEP=1
HOSTSOLID2D,SOLID2D,MEM2D
*NODE
*ELEMENT, TYPE=CAX4, ELSET=HOSTSOLID2D1
*ELEMENT, TYPE=CAX4, ELSET=SOLID2D1
*ELEMENT, TYPE=SFMAX1, ELSET=MEM2D1
*SOLID SECTION,ELSET=HOSTSOLID2D1,MATERIAL=STEEL
*SURFACE SECTION,ELSET=MEM2D1
*REBAR LAYER
REB101,0.005,0.31416,0,MAT2,50,1
REB102,0.005,0.31416,0,MAT2,30,1
*SOLID SECTION,ELSET=SOLID2D1,MATERIAL=STEEL2
*EMBEDDED ELEMENT,HOST ELSET=HOSTSOLID2D1,ROUND OFF TOLERANCE=0.005
SOLID2D1,MEM2D1
*BOUNDARY
1,1,2
5,1,2
101,1,2
105,1,2
*FILE FORMAT, ZERO INCREMENT
*STEP,nlgeom
*STATIC
1.0,1.0
*CLOAD
4,2,-2.0E6
8,2,-2.0E6
104,2,-2.0E6
108,2,-2.0E6
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=MEM2D,REBAR
S
LE
*ELEMENT OUTPUT,ELSET=MEM2D1,REBAR
S
LE
*ELEMENT OUTPUT,ELSET=SOLID2D
S
LE
*ELEMENT OUTPUT,ELSET=SOLID2D1
S
LE
*ELEMENT OUTPUT,ELSET=HOSTSOLID2D
S
LE
*ELEMENT OUTPUT,ELSET=HOSTSOLID2D1
S
LE
*EL FILE,ELSET=MEM2D,REBAR
S
E
*EL FILE,ELSET=MEM2D1,REBAR
S
E
*EL FILE,ELSET=SOLID2D
S
E
*EL FILE,ELSET=SOLID2D1
S
E
*EL FILE,ELSET=HOSTSOLID2D
S
E
*EL FILE,ELSET=HOSTSOLID2D1
S
E
*EL PRINT,ELSET=MEM2D,REBAR
S
E
*EL PRINT,ELSET=SOLID2D
S
E
*EL PRINT,ELSET=HOSTSOLID2D
S
E
*END STEP