*HEADING
Import analysis: explicit-standard
*IMPORT,UPDATE=NO,STATE=YES
EALL,
*RESTART, WRITE
*FILE FORMAT, ZERO INC
**
*AMPLITUDE, NAME=RAMP
0.0,0.0,1.0,1.0
*STEP, NLGEOM
Forth (and final) springback analysis
*STATIC
0.1,1.0
*BOUNDARY,OP=NEW
BUILTIN,1,3
*CLOAD, OP=NEW
*OUTPUT, FIELD
*ELEMENT OUTPUT, VARIABLE=PRESELECT
*NODE OUTPUT, VARIABLE=PRESELECT
*NODE FILE, NSET=TIP
U,
*EL FILE, ELSET=EALL
S,EE,LE,PE
*MONITOR, DOF=3, NODE=50
*END STEP