*Heading
STANDARD-TO-EXPLICIT IMPORT
*IMPORT, STATE=YES, UPDATE=NO
SOLID, FLUID, INF
*PARAMETER
f=15
omega=2*3.14159*f
*AMPLITUDE,NAME=SINE,DEF=PERIODIC
1,<omega>,-0.005,0.0
0,1,0,0
*SURFACE,NAME=SOLID
3,S2
4,S2
*SURFACE,NAME=FLUID
5,S1
6,S1
7,S1
8,S1
*TIE,NAME=COUPLE
SOLID,FLUID
*NSET, NSET=BACK_S
*BOUNDARY
BACK_S,1,3
*STEP
*DYNAMIC, EXPLICIT
,0.005
*BOUNDARY,AMP=SINE
FRONT_F,8,,1e3
*output,field,variable=preselect
*output,history,variable=preselect
** Output Request for QA Purposes **
*OUTPUT,FIELD,NUMBER INTERVAL=1
*NODE OUTPUT,NSET=QA_TEST
U
*OUTPUT,HISTORY,TIME INTERVAL=0.005
*ENERGY OUTPUT,VARIABLES=PRESELECT
*******
*END STEP