*HEADING
 Transfer from Standard to Explicit : MPC link
 - Explicit analysis
 [references xs_s_cps4r_mpclink]
*IMPORT,UPDATE=NO,STATE=YES
ELALL,
*RESTART,TIMEMARKS=YES,WRITE,NUM=1
*MPC
LINK, 2,5
LINK, 3,8
**
** STEP #1
**
*STEP
*DYNAMIC,EXPLICIT
,0.1
*BOUNDARY,TYPE=VELOCITY
LEFT,  1,1,
BOTTOM,2,2
RIGHT, 1,1, 5.0
*FILE OUTPUT,TIMEMARKS=YES,NUM=1
*NODE FILE
U,
***OUTPUT,HISTORY,TIME INTERVAL=2.5E-3
***ELEMENT OUTPUT,ELSET=ELALL
**S,LE
******
*elset,elset=QA_TEST
*NSET,NSET=QA_TEST,ELSET=QA_TEST
*output,field,variable=preselect
*output,history,variable=preselect
** Output Request for QA Purposes **
*OUTPUT,FIELD,NUMBER INTERVAL=1
*NODE OUTPUT,NSET=QA_TEST
U
*ELEMENT OUTPUT,ELSET=QA_TEST
LE
*OUTPUT,HISTORY,TIME INTERVAL=0.1
*ENERGY OUTPUT,VARIABLES=PRESELECT
*******
*END STEP