*HEADING
 SYMMETRIC RESULTS TRANSFER FOR TIRE ROLLING ON 1.5m DRUM
 3D FULL TIRE MODEL
 STEP 0: TRANSFER TIRE FOOTPRINT RESULTS FROM
         TIRETRANSFER_SYMM_DRUM
 STEP 1: BRING TRANSFERRED RESULTS TO EQUILIBRIUM
 UNITS: KG, M
*RESTART,WRITE,FREQ=100
*SYMMETRIC MODEL GENERATION,REFLECT=LINE,ELEMENT=15000,NODE=15000,TRANSPORT
*SYMMETRIC RESULTS TRANSFER,STEP=3,INC=1
**************************************************
*STEP,INC=100,NLGEOM=YES
 1:  BRING TRANSFERRED RESULTS TO EQUILIBRIUM
*STATIC, LONG TERM, DIRECT
 1.0, 1.0
*BOUNDARY,OP=NEW
 RIM,  1, 6
 DRUM, 1, 2
 DRUM, 4, 6
*DSLOAD,OP=NEW
 INSIDE, P, 200.E3
*CLOAD,OP=NEW
 DRUM, 3, 3300.
*NODE PRINT,NSET=DRUM,FREQ=1
 U,
 RF,
*EL PRINT,FREQ=0
*OUTPUT,FIELD,FREQ=1
*ELEMENT OUTPUT
 S,LE
*ELEMENT OUTPUT,REBAR
 S,LE
*NODE OUTPUT
 U,
*OUTPUT,HISTORY,VAR=PRESELECT,FREQ=1
*NODE OUTPUT, NSET=DRUM
 U, RF
*NODE OUTPUT, NSET=RIM
 U, RF
*END STEP