*HEADING
 SYMMETRIC RESULTS TRANSFER FOR TIRE MODEL
 3D HALF TIRE MODEL
 STEP 0: TRANSFER TIRE INFLATION RESULTS FROM
 STEP 1: BRING TRANSFERRED AXISYMMETRIC RESULTS
         TO EQUILIBRIUM
 STEP 2: FOOTPRINT ANALYSIS (DISPLACEMENT CONTROL)
 STEP 3: FOOTPRINT ANALYSIS (LOAD CONTROL)
 UNITS: KG, M
*RESTART,WRITE,FREQ=100
*NODE,NSET=ROAD
*SYMMETRIC MODEL GENERATION,REVOLVE,ELEMENT=1000,
NODE=1000,TRANSPORT
120., 6,,g
 40., 8,,g
 40.,20,,g
 40., 8,,g
120., 6,,g
*SYMMETRIC RESULTS TRANSFER, STEP=1
*SURFACE,TYPE=CYLINDER,NAME=SROAD
 START, -0.3, 0.
 LINE,   0.3, 0.
*RIGID BODY,REF NODE=ROAD,ANALYTICAL SURFACE=SROAD
*CONTACT PAIR,INTERACTION=SRIGID
 TREADSURF, SROAD
*SURFACE INTERACTION,NAME=SRIGID
*SURFACE BEHAVIOR, AUGMENTED LAGRANGE
*FRICTION
 0.0
*NSET,NSET=SYM1
**
** NODE SETS ASYMA,ASYMB,ASYMC, and ASYMD
** USED FOR ANTI_SYMMETRY BC's
**
*NSET,NSET=ASYMA,GENERATE,UNSORTED
*NSET,NSET=ASYMB,GENERATE,UNSORTED
*NSET,NSET=ASYMC,GENERATE,UNSORTED
*NSET,NSET=ASYMD,GENERATE,UNSORTED
*EQUATION
 ASYMA, 1, 1.0, ASYMB, 1,  1.0
*EQUATION
 ASYMA, 2, 1.0, ASYMB, 2,  1.0
*EQUATION
 ASYMC, 3, 1.0, ASYMD, 3, -1.0
********************************************
*STEP,INC=100,NLGEOM=YES
 1:  BRING TRANSFERRED RESULTS TO EQUILIBRIUM
*STATIC, LONG TERM
 1.0, 1.0
*BOUNDARY,OP=NEW
 RIM,  1, 6
 ROAD, 1, 6
 SYM1, 1, 2
*DSLOAD,OP=NEW
 INSIDE, P, 200.E3
*NODE PRINT,NSET=ROAD,FREQ=0
 U,
 RF,
*EL PRINT,FREQ=0
*OUTPUT,FIELD,FREQ=1
*ELEMENT OUTPUT
 S,LE
*ELEMENT OUTPUT,REBAR
 S,LE
*NODE OUTPUT
 U
*CONTACT OUTPUT,VAR=PRESELECT
*OUTPUT,HISTORY,VAR=PRESELECT,FREQ=1
*NODE OUTPUT, NSET=ROAD
 U,RF,CF
*END STEP
******************************************
*STEP,INC=100,NLGEOM=YES
 2:  FOOTPRINT (Displacement controlled)
*STATIC, LONG TERM
 0.2, 1.0
*BOUNDARY,OP=NEW
 RIM,  1, 6
 ROAD, 1, 2
 ROAD, 4, 6
 SYM1, 1, 2
 ROAD, 3, , 0.02
*END STEP
****************************************
*STEP,INC=100,NLGEOM=YES
 3:  FOOTPRINT (Load controlled)
*STATIC, LONG TERM
 1.0, 1.0
*BOUNDARY,OP=NEW
 RIM,  1, 6
 ROAD, 1, 2
 ROAD, 4, 6
 SYM1, 1, 2
*CLOAD, OP=NEW
 ROAD, 3, 1650.
*END STEP