*HEADING
TEST OF AMPLITUDES IN RESTARTS                                     XAMP2
ONLY THE VALUES OF THE PRESCRIBED BOUNDARY CONDITIONS AND LOADS
ARE TO BE CHECKED FROM THIS ANALYSIS TO VERIFY THE AMPLITUDE SPECIFICATIONS.
THE ANALYSIS IS RESTARTED WITHIN STEP 1 USING AN ENDSTEP PARAMETER. ALL
DEFINITIONS OF LOADS AND BOUNDARY CONDITIONS ARE SET TO ZERO IN THE
SUBSEQUENT STEP. THIS TESTS THE ABILITY TO READ THE AMPLITUDE CURVES AT
ANY TIME IN THE STEP AND RAMP THE VALUES TO THE NEXT VALUE.
*RESTART,READ,STEP=1,INTERVAL=4,ENDSTEP
*STEP
REMOVE (LINEARLY) LOADS AND BOUNDARY CONDITIONS
*DYNAMIC,EXPLICIT
,0.08
*CLOAD,OP=NEW
*BOUNDARY,OP=NEW
BCSET,1,3
*FILE OUTPUT,NUM=5
*NODE FILE,NSET=BCSET
U,
*END STEP