*HEADING
Explicit verification for meshed general section
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
*PART, NAME=LINEARMESHED
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B31, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=MESHED,ELSET=EALL
0., 0., -1.
*INCLUDE,INPUT=meshedsect_i_ortho.bsp
*END PART
*PART, NAME=QUADRATICMESHED
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B32, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=MESHED,ELSET=EALL
0., 0., -1.
*INCLUDE,INPUT=meshedsect_i_ortho.bsp
*END PART
*ASSEMBLY, NAME=ASSEMBLY
*INSTANCE,NAME=LINEARMESHED_A, PART=LINEARMESHED
*END INSTANCE
*INSTANCE,NAME=QUADRATICMESHED_A, PART=QUADRATICMESHED
*END INSTANCE
*END ASSEMBLY
*BOUNDARY
ASSEMBLY.LINEARMESHED_A.1, 1, 6
ASSEMBLY.QUADRATICMESHED_A.1, 1, 6
*NSET, NSET=QA_TEST_NALL
ASSEMBLY.LINEARMESHED_A.11
ASSEMBLY.QUADRATICMESHED_A.11
*ELSET, ELSET=QA_TEST_EALL
ASSEMBLY.LINEARMESHED_A.1
ASSEMBLY.QUADRATICMESHED_A.1
*STEP
*DYNAMIC, EXPLICIT
,1.E-1
*CLOAD
ASSEMBLY.LINEARMESHED_A.11,2,2.5E+5
ASSEMBLY.QUADRATICMESHED_A.11,2,2.5E+5
*FILE OUTPUT, NUMBER=4
*EL FILE
S,LE
*OUTPUT,FIELD,NUMBER=4, TIMEMARKS=YES
*NODE OUTPUT, NSET=QA_TEST_NALL
U,
*ELEMENT OUTPUT,ELSET=QA_TEST_EALL
S,LE
*OUTPUT, HISTORY,FREQ=10
*NODE OUTPUT, NSET=QA_TEST_NALL
U,
*ELEMENT OUTPUT,ELSET=QA_TEST_EALL
S,LE,
*END STEP