*HEADING
 Transfer from Explicit to Standard : Plasticity Test for CPS4R element
 - Standard Analysis
 - Plastic material
*IMPORT,STEP=1,INT=5,UPDATE=NO,STATE=YES
 PS,
 PS2,
 PS3,
*RESTART, WRITE, FREQ=100
**
*BOUNDARY
XBOUN,1
XSYMM,1
YSYMM,2
*STEP,INC=500,NLGEOM
*STATIC
 0.00001, 1.,1e-6,0.01
*BOUNDARY
TOP,2,2,2.5
*PRINT,FREQ=1
***EL FILE
** PEEQ,MISES
*EL PRINT
PEEQ,
MISES,
*NODE FILE,FREQ=100
 COORD,
*OUTPUT,HISTORY,VARIABLE=PRESELECT
*OUTPUT,FIELD
*NODE OUTPUT
 COORD,U
*ELEMENT OUTPUT
S,LE,PE,PEEQ
*END STEP