*Restart, read, step=2
*Step, name=Step-3, perturbation
*Steady State Dynamics, frequency scale=LINEAR, interval=range
30., 40., 3,
*Cload
Part-1-1.17, 2, 1.e10
**
** OUTPUT REQUESTS
**
*Output, field
*node output, nset=ams_set
U
*End Step