*Heading
** Job name: driveshaft Model name: Driveshaft
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Centershaft
*End Part
**
*Part, name=Inputshaft
*End Part
**
*Part, name=Outputshaft
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Centershaft-1, part=Centershaft
*Node
*Element, type=B31
** Region: (shaft_section:Picked), (Beam Orientation:Picked)
*Elset, elset=_PickedSet2, internal, generate
** Section: shaft_section  Profile: Profile-1
*Beam General Section, elset=_PickedSet2, poisson = 0.3, density=7000., section=CIRC
0.1
0.,0.,-1.
 2e+11, 7.6e+10
*End Instance
**
*Instance, name=Inputshaft-1, part=Inputshaft
*Node
*Element, type=B31
** Region: (shaft_section:Picked), (Beam Orientation:Picked)
*Elset, elset=_PickedSet2, internal
** Section: shaft_section  Profile: Profile-1
*Beam General Section, elset=_PickedSet2, poisson = 0.3, density=7000., section=CIRC
0.1
0.,0.,-1.
 2e+11, 7.6e+10
*End Instance
**
*Instance, name=Outputshaft-1, part=Outputshaft
*Node
*Element, type=B31
** Region: (shaft_section:Picked), (Beam Orientation:Picked)
*Elset, elset=_PickedSet2, internal
** Section: shaft_section  Profile: Profile-1
*Beam General Section, elset=_PickedSet2, poisson = 0.3, density=7000., section=CIRC
0.1
0.,0.,-1.
 2e+11, 7.6e+10
*End Instance
**
*Nset, nset=_PickedSet8, internal, instance=Inputshaft-1
*Nset, nset=QA_TEST, internal, instance=Inputshaft-1
*Nset, nset=_PickedSet9, internal, instance=Outputshaft-1
*Nset, nset=_PickedSet18, internal, instance=Outputshaft-1
*Orientation, name="Datum csys-4"
*Orientation, name="Datum csys-5"
*Orientation, name="Datum csys-2"
*Orientation, name="Datum csys-3"
**
** CONNECTORS
**
*Element, type=CONN3D2, elset=_Connector_centershaft_outputshaft_CnSet_
1, Centershaft-1.4, Outputshaft-1.1
*Connector Section, elset=_Connector_centershaft_outputshaft_CnSet_
UJoint,
"Datum csys-4", "Datum csys-5"
*Element, type=CONN3D2, elset=_Connector_inputshaft_centershaft_CnSet_
2, Inputshaft-1.3, Centershaft-1.1
*Connector Section, elset=_Connector_inputshaft_centershaft_CnSet_
UJoint,
"Datum csys-2", "Datum csys-3"
*End Assembly
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, nlgeom=YES
*Static
0.1, 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary
_PickedSet8, 1, 1
_PickedSet8, 2, 2
_PickedSet8, 3, 3
_PickedSet8, 4, 4, 6.28
_PickedSet8, 5, 5
_PickedSet8, 6, 6
** Name: BC-2 Type: Displacement/Rotation
*Boundary
_PickedSet9, 1, 1
_PickedSet9, 2, 2
_PickedSet9, 3, 3
_PickedSet9, 5, 5
_PickedSet9, 6, 6
**
** LOADS
**
** Name: Load-1   Type: Moment
*Cload
_PickedSet18, 4, 1000.
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*OUTPUT,field, freq=10000
*NODE OUTPUT, nset=QA_TEST
u,
**
** HISTORY OUTPUT: H-Output-1
**
*OUTPUT, history
*node output, nset=QA_TEST
ur1,
*El Print, freq=999999
*Node Print, freq=999999
*End Step