*Heading
**
*Node, nset=projectile
*Element, type=C3D8R, elset=projectile
*solidsection, elset=projectile, controls=EC-1, material=steel
**
*Node, nset=plate
*Element, type=C3D8R, elset=plate
*solidsection, elset=plate, controls=EC-1, material=steel
**
*Nset, nset=ysymm_nodes
*Nset, nset=fixed_nodes
*Elset, elset=erode, generate
*Elset, elset=erode
**
*sectioncontrols, name=EC-1, hourglass=ENHANCED, kinematicsplit=ORTHOGONAL,distortion control,length ratio=0.1
***material, name=MATERIAL-1
***density
**7800.,
***elastic
**2.078E+11, 0.3
***plastic
**1.22E+09, 0.
**2.44E+09, 1.
***shear failure
**1.0,
*material,name=steel
*include,input=erode_material.inp
***material,name=aluminum
***include,input=aluminum.abaqus
*boundary
ysymm_nodes, YSYMM
*boundary
fixed_nodes, PINNED
*initialconditions, type=VELOCITY
projectile, 1,  684.0
projectile, 2,  0.0
projectile, 3, -1879.4
*surface,type=element,name=surf1
erode,interior
*Step, name=Step-1
*dynamic, explicit
, 6E-06
*bulkviscosity
*contact, op=NEW
*contactinclusions
surf1,
*contact controls assignment, nodal erosion=no
*nset, nset=QA_TEST
ysymm_nodes
*output, field, num=1, timemarks=yes
*nodeoutput,nset=QA_TEST
 U,
*output, field, num=12
*nodeoutput
U,V,A
*elementoutput
PEEQ, S, STATUS
*contactoutput
CFORCE, CSTRESS
*output, history, variable=PRESELECT
*endstep