*Heading
** Job name: fastener_projdir_s4 Model name: Model-1
**
** PARTS
**
*Preprint, model=yes, history=yes
*Part, name=Part-2
*End Part
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Part-2-1, part=Part-2
*Node
*Element, type=S4
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Shell Section, elset=_I1, material=Material-1
0.02, 5
*End Instance
**
*Instance, name=Part-2-2, part=Part-2
*Node
*Element, type=S4
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Shell Section, elset=_I1, material=Material-1
0.02, 5
*End Instance
**
*Instance, name=Part-2-3, part=Part-2
*Node
*Element, type=S4
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Shell Section, elset=_I1, material=Material-1
0.02, 5
*End Instance
**
*Instance, name=Part-2-4, part=Part-2
*Node
*Element, type=S4
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Shell Section, elset=_I1, material=Material-1
0.02, 5
*End Instance
**
*Instance, name=Part-2-5, part=Part-2
*Node
*Element, type=S4
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Shell Section, elset=_I1, material=Material-1
0.02, 5
*End Instance
*Nset, nset=refNode1, internal, instance=Part-2-1
*Nset, nset=refNode2, internal, instance=Part-2-2
*Nset, nset=refNode3, internal, instance=Part-2-3
*Nset, nset=refNode4, internal, instance=Part-2-4
*Nset, nset=refNode5, internal, instance=Part-2-5
*Nset, nset=refNode
 refNode1, refNode2, refNode3, refNode4, refNode5
*Nset, nset=_PickedSet35, internal, instance=Part-2-1, generate
*Nset, nset=_PickedSet35, internal, instance=Part-2-2, generate
*Nset, nset=_PickedSet35, internal, instance=Part-2-3, generate
*Nset, nset=_PickedSet35, internal, instance=Part-2-5, generate
*Nset, nset=_PickedSet35, internal, instance=Part-2-4, generate
*Elset, elset=_TopSurf_SPOS, internal, instance=Part-2-1, generate
*Elset, elset=_TopSurf_SPOS, internal, instance=Part-2-2, generate
*Elset, elset=_TopSurf_SPOS, internal, instance=Part-2-3, generate
*Elset, elset=_TopSurf_SPOS, internal, instance=Part-2-5, generate
*Elset, elset=_TopSurf_SPOS, internal, instance=Part-2-4, generate
*Surface, type=ELEMENT, name=TopSurf
_TopSurf_SPOS, SPOS
*Elset, elset=_TopSurf1_SPOS, internal, instance=Part-2-1, generate
*Surface, type=ELEMENT, name=TopSurf1
_TopSurf1_SPOS, SPOS
*Elset, elset=_TopSurf2_SPOS, internal, instance=Part-2-2, generate
*Surface, type=ELEMENT, name=TopSurf2
_TopSurf2_SPOS, SPOS
*Elset, elset=_TopSurf3_SPOS, internal, instance=Part-2-3, generate
*Surface, type=ELEMENT, name=TopSurf3
_TopSurf3_SPOS, SPOS
*Elset, elset=_TopSurf4_SPOS, internal, instance=Part-2-4, generate
*Surface, type=ELEMENT, name=TopSurf4
_TopSurf4_SPOS, SPOS
*Elset, elset=_TopSurf5_SPOS, internal, instance=Part-2-5, generate
*Surface, type=ELEMENT, name=TopSurf5
_TopSurf5_SPOS, SPOS
*End Assembly
*Fastener, interaction name=inter-1, property=prop-1, search radius=10.,
 reference node set=refNode1, radius of influence=0.6
 TopSurf1,
*Fastener, interaction name=inter-2, property=prop-1, reference node set=refNode2, search radius=10.
 TopSurf2,
*Fastener, interaction name=inter-3, property=prop-1, reference node set=refNode3, search radius=10.
 TopSurf3,
*Fastener, interaction name=inter-4, property=prop-1, reference node set=refNode4, search radius=10.
 TopSurf4,
*Fastener, interaction name=inter-5, property=prop-1, reference node set=refNode5, search radius=10.
 TopSurf5,
*Fastener Property, name=prop-1
**
** MATERIALS
**
*Material, name=Material-1
*Elastic
 2e+11, 0.3
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1
Load
*Static
 0.25, 1.
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary
_PickedSet35, 1, 3
**
** LOADS
**
** Name: Load-1   Type: Pressure
*Dsload
TopSurf, P, -1.e3
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
 U,
*Output, history
*Interaction Output, nset=refNode
 FTF3,
*El Print, freq=0
*Node Print, freq=0
*Interaction Print, name=inter-1
 FTF,
*Interaction Print, name=inter-2
 FTF,
*Interaction Print, name=inter-3
 FTF,
*Interaction Print, name=inter-4
 FTF,
*Interaction Print, name=inter-5
 FTF,
*End Step