*Heading
*Restart, read, step=8
** ----------------------------------------------------------------
**
** STEP: Step-9
**
*Step, name=Step-9, nlgeom
 unload
*Static
 0.1, 1., 1e-05, 0.2
*Boundary
 EdgeCube,  1,6
 KinRefAll, 1,6
*Interaction Print, name=Inter-1
 FTF,
*Interaction Print, nset=RefNodePX
 FTF,
*End Step