*HEADING
 IMPORT ROLLING TIRE: FULL TIRE MODEL
 UNITS: KG, M
*RESTART,WRITE,FREQ=100
*SYMMETRIC MODEL GENERATION,REFLECT=LINE,ELEMENT=100000,NODE=100000,TRANSPORT
*SYMMETRIC RESULTS TRANSFER,STEP=3
**************************************************
*STEP,NLGEOM=YES
 1:  BRING TRANSFERRED RESULTS TO EQUILIBRIUM
*STATIC, DIRECT, LONGTERM
 1.0, 1.0
*BOUNDARY,OP=NEW
 RIM,  1, 6
 ROAD, 1, 2
 ROAD, 4, 6
*DSLOAD,OP=NEW
 INSIDE, P, 200.E3
*CLOAD,OP=NEW
 ROAD, 3, 3300.
*NODE PRINT,FREQ=0
*EL PRINT,FREQ=0
*OUTPUT,FIELD,FREQ=1
*ELEMENT OUTPUT
 S,LE
*NODE OUTPUT
 U
*CONTACT OUTPUT,VAR=PRE
*OUTPUT,HISTORY,FREQ=1
*NODE OUTPUT, NSET=ROAD
 U, RF, UR1,UR2,UR3,RM1,RM2,RM3
*NODE OUTPUT, NSET=RIM
 U, RF, UR1,UR2,UR3,RM1,RM2,RM3
*ENERGY OUTPUT,VAR=PRE
*END STEP