*Heading
 LCA with Substructure and Bushing Connector Analysis -- Load Case 2
**
** LCA substructure usage
**
*Node, nset=LCA-BallJoint
*Node, nset=LCA-RearBushing
*Node, nset=LCA-FrontBushing
**
*Element, Type=Z1, Elset=LCA, File=LCA
*Substructure Property, Elset=LCA
**
** Front Bushing
**
*Node, nset=FrontBushing
*Element, Type=CONN3D2, Elset=FrontBushing
*Connector Section, elset=FrontBushing, behavior=FrontBushing
Bushing,
FB-CSYS-1, FB-CSYS-2
**
** Rear Bushing
**
*Node, nset=RearBushing
*Element, Type=CONN3D2, Elset=RearBushing
*Connector Section, elset=RearBushing, behavior=RearBushing
Bushing,
RB-CSYS-1, RB-CSYS-2
**
** CSYS definitions
**
*Orientation, name=FB-CSYS-1
*Orientation, name=FB-CSYS-2
*Orientation, name=RB-CSYS-1
*Orientation, name=RB-CSYS-2
**
**
*Connector Behavior, name=FrontBushing
*Connector Elasticity, nonlinear, component=1
*Connector Elasticity, nonlinear, component=2
*Connector Elasticity, nonlinear, component=3
*Connector Elasticity, nonlinear, component=4
*Connector Elasticity, nonlinear, component=6
*Connector Elasticity, nonlinear, component=5, independent components=CONSTITUTIVE MOTION
*Connector Behavior, name=RearBushing
*Connector Elasticity, nonlinear, component=2
*Connector Elasticity, nonlinear, component=3
*Connector Elasticity, nonlinear, component=4
*Connector Elasticity, nonlinear, component=5
*Connector Elasticity, nonlinear, component=6
*Connector Elasticity, nonlinear, component=1, independent components=CONSTITUTIVE MOTION
**
** BOUNDARY CONDITIONS
**
*Boundary
 FrontBushing, ENCASTRE
 RearBushing, ENCASTRE
**
** STEP: Step-1
**
*Step, name=Step-1, nlgeom=YES
Load Case 2 -- Step-1 -- Lift Ball Joint
*Static
 0.1, 1.0, 1.0e-05, 1.0
**
** Loads
**
*Boundary
 LCA-BallJoint, 3, 3, -60.
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT
**
*Substructure Path, Enter Element=1
*Output, field, frequency=999
*Node Output
 U,
*substructure Path, Leave
**
*Output, field, frequency=999
*Node Output
 U,
**
** HISTORY OUTPUT
**
*Output, history
*Element Output, elset=FrontBushing
CTF1, CTF2, CTF3, CTM1, CTM2, CTM3, CU1, CU2, CU3, CUR1, CUR2, CUR3
**
*Element Output, elset=RearBushing
CTF1, CTF2, CTF3, CTM1, CTM2, CTM3, CU1, CU2, CU3, CUR1, CUR2, CUR3
**
*Node Output, nset=LCA-BallJoint
U1, U2, U3, UR1, UR2, UR3
**
*Node Output, nset=RearBushing
RF1, RF2, RF3, RM1, RM2, RM3
**
*Node Output, nset=FrontBushing
RF1, RF2, RF3, RM1, RM2, RM3
**
*End Step
**
** STEP: Step-2
**
*Step, name=Step-2, nlgeom=YES
Load Case 2 -- Step-2 -- Load Ball Joint
*Static
 0.1, 1.0, 1.0e-05, 1.0
*Cload
 LCA-BallJoint, 1, -1000.
*End Step