*Heading
*preprint,model=yes,history=yes
*NODE, NSET=NALL
*ELEMENT, TYPE=MASS, ELSET=MASS
*MASS, ELSET=MASS
1.,
*ELEMENT, TYPE=ROTARYI, ELSET=ROT
*ROTARY INERTIA, ELSET=ROT
1.,1.,1.
*ORIENTATION, NAME=ORIENT1
*ORIENTATION, NAME=ORIENT2
*ELEMENT, TYPE=CONN3D2, ELSET=CONN1
*ELEMENT, TYPE=CONN3D2, ELSET=CONN2
*CONNECTOR SECTION, ELSET=CONN1
BEAM,
*CONNECTOR SECTION, ELSET=CONN2
ACCELEROMETER,
ORIENT1,ORIENT2
*BOUNDARY
1,1,3,0.0
3,1,6,0.0
*****************************************************************
*NODE, NSET=NALL10
*ELEMENT, TYPE=MASS, ELSET=MASS10
*MASS, ELSET=MASS10
1.,
*ELEMENT, TYPE=ROTARYI, ELSET=ROT10
*ROTARY INERTIA, ELSET=ROT10
1.,1.,1.
*ELEMENT, TYPE=CONN3D2, ELSET=CONN10
*ELEMENT, TYPE=CONN3D2, ELSET=CONN20
*CONNECTOR SECTION, ELSET=CONN10
BEAM,
*CONNECTOR SECTION, ELSET=CONN20
ACCELEROMETER,ROTATION-ACCELEROMETER
ORIENT1,ORIENT2
*BOUNDARY
100,1,3,0.0
300,1,6,0.0
**********************************************************
*NSET, NSET=OUT
*STEP, NAME=STEP-1
*DYNAMIC,EXPLICIT,DIRECT
1.E-4,1.0,
*BOUNDARY, TYPE=VELOCITY
100,6,6,1.0
*CONNECTOR MOTION, TYPE=VELOCITY
CONN2,2,10.0
*OUTPUT, FIELD, N=1
*NODEOUTPUT
U,
*OUTPUT, HISTORY, FREQ=100
*NODE OUTPUT, NSET=OUT
U,V
*ELEMENT OUTPUT, ELSET=CONN2
CU,CV
*ELEMENT OUTPUT, ELSET=CONN20
CU,CV
*ENERGY OUTPUT
ALLKE,ALLIE,ALLSE,ALLWK,ETOTAL
*ENDSTEP