*HEADING
CONNECTOR FUNCTIONALITY VERIFICATION - CARTESIAN, CARDAN & ROTATION
**
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
**
******************************
**  CONN3D2 NODES/ELEMENTS  **
******************************
**
*NODE,NSET=NALL3D
**
*ELEMENT,TYPE=CONN3D2,ELSET=TESTTF
*ELEMENT,TYPE=CONN3D2,ELSET=TESTTD
*ELEMENT,TYPE=CONN3D2,ELSET=TESTRF
*ELEMENT,TYPE=CONN3D2,ELSET=TESTRD
*ELEMENT,TYPE=CONN3D2,ELSET=TESTROTF
*ELEMENT,TYPE=CONN3D2,ELSET=TESTROTD
**
*ELSET,ELSET=TEST
TESTTF,TESTTD,TESTRF,TESTRD,TESTROTF,TESTROTD
*ELEMENT,TYPE=MASS,ELSET=MASS
*ELEMENT,TYPE=ROTARYI,ELSET=ROT
**
*MASS,ELSET=MASS
1.E-4,
*ROTARY INERTIA,ELSET=ROT,ORIENTATION=ORIGLOB
1.E-3,1.E-3,1.E-3
**
***********************************************************
** DISPLACEMENT LIMITED CONNECTOR FAILURE FOR CARTESIAN  **
***********************************************************
**
*CONNECTOR SECTION,ELSET=TESTTD,BEHAVIOR=TBTD
CARTESIAN,
ORIGLOB,
**
*ORIENTATION,SYS=RECT,NAME=ORIGLOB
**
*CONNECTOR BEHAVIOR,NAME=TBTD
*CONNECTOR ELASTICITY,COMPONENT=1
*CONNECTOR ELASTICITY,COMPONENT=2
*CONNECTOR ELASTICITY,COMPONENT=3
*CONNECTOR FAILURE,COMPONENT=2,RELEASE=1
**
*BOUNDARY
11,1,6
12,4,6
**
*********************************************************
** DISPLACEMENT LIMITED CONNECTOR FAILURE FOR CARDAN   **
*********************************************************
**
*CONNECTOR SECTION,ELSET=TESTRD,BEHAVIOR=TBRD
CARDAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBRD
*CONNECTOR ELASTICITY,COMPONENT=4
*CONNECTOR ELASTICITY,COMPONENT=6
*CONNECTOR FAILURE,COMPONENT=6,RELEASE=4
**
*BOUNDARY
31,1,6
32,1,3
32,5,5
**
****************************************************
** FORCE LIMITED CONNECTOR FAILURE FOR CARTESIAN  **
****************************************************
**
*CONNECTOR SECTION,ELSET=TESTTF,BEHAVIOR=TBTF
CARTESIAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBTF
*CONNECTOR ELASTICITY,COMPONENT=1
*CONNECTOR ELASTICITY,COMPONENT=2
*CONNECTOR ELASTICITY,COMPONENT=3
*CONNECTOR FAILURE,COMPONENT=2,RELEASE=1
**
*BOUNDARY
1,1,6
2,4,6
**
**************************************************
** FORCE LIMITED CONNECTOR FAILURE FOR CARDAN   **
**************************************************
**
*CONNECTOR SECTION,ELSET=TESTRF,BEHAVIOR=TBRF
CARDAN,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBRF
*CONNECTOR ELASTICITY,COMPONENT=4
*CONNECTOR ELASTICITY,COMPONENT=6
*CONNECTOR FAILURE,COMPONENT=6,RELEASE=4
**
*BOUNDARY
21,1,6
22,1,3
22,5,5
**
***********************************************************
** DISPLACEMENT LIMITED CONNECTOR FAILURE FOR ROTATION   **
***********************************************************
**
*CONNECTOR SECTION,ELSET=TESTROTD,BEHAVIOR=TBROTD
ROTATION,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBROTD
*CONNECTOR ELASTICITY,COMPONENT=4
*CONNECTOR ELASTICITY,COMPONENT=6
*CONNECTOR FAILURE,COMPONENT=6,RELEASE=4
**
*BOUNDARY
51,1,6
52,1,3
52,5,5
**
****************************************************
** FORCE LIMITED CONNECTOR FAILURE FOR ROTATION   **
****************************************************
**
*CONNECTOR SECTION,ELSET=TESTROTF,BEHAVIOR=TBROTF
ROTATION,
ORIGLOB,
**
*CONNECTOR BEHAVIOR,NAME=TBROTF
*CONNECTOR ELASTICITY,COMPONENT=4
*CONNECTOR ELASTICITY,COMPONENT=6
*CONNECTOR FAILURE,COMPONENT=6,RELEASE=4
**
*BOUNDARY
41,1,6
42,1,3
42,5,5
**
*AMPLITUDE,NAME=VP,DEFINITION=SMOOTH STEP,SMOOTH=0.05
0.,0.,0.01,1.0
**
*NSET,NSET=NALL
NALL3D,
*ELSET,ELSET=TEST
TESTTF,TESTTD,TESTRF,TESTRD,TESTROTF,TESTROTD
**
*ELSET,ELSET=QA_TEST_TEST
TEST,
*NSET,NSET=QA_TEST_NALL
NALL,
**
*STEP,NLGEOM=YES
CONNECTOR TEST STEP - CONNECTOR FAIL
*STATIC,direct
1.0E-4,0.01
**
*BOUNDARY,AMPLITUDE=VP
 2,1,3,0.1
12,1,3,0.1
22,4,4,0.1
32,4,4,0.1
22,6,6,0.1
32,6,6,0.1
42,4,4,0.1
52,4,4,0.1
**
*OUTPUT,HISTORY,VARIABLE=PRESELECT
*ELEMENT OUTPUT,ELSET=TEST
CFAILST,CEF,
*ENDSTEP