*HEADING
ABAQUS/STANDARD SELF CONTACT: JOUNCE BUMPER WITH CAX3 ELEMENTS
IMPORT SOLUTION OF INTERFERENCE FIT RESOLUTION AT END OF STEP ONE FROM
selfcontact_bump_surf.inp
**
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
*IMPORT, UPDATE=NO, STATE=YES, STEP=1
ALLFEM,
*NSET, NSET=BOTDIE
*NSET, NSET=TOPDIE
*NSET, NSET=SHAFTDIE
*SURFACE INTERACTION, NAME=INTPROP
1.,
*FRICTION
0.05,
**
** Boundary conditions
**
*BOUNDARY
1000, 1, 1
1000, 6, 6
1001, ENCASTRE
1002, ENCASTRE
**
** History definition
**
*STEP, INC=200, NLGEOM, UNSYMM=YES, CONVERT SDI=YES
*STATIC
 0.1, 1.0
*BOUNDARY
1000, 2, 2, 42.
**
** Output requests
**
*OUTPUT, FIELD, OP=NEW,FREQ=10
*NODE OUTPUT
U, V, A, RF
*ELEMENT OUTPUT
S, PE, PEEQ, LE
*CONTACT OUTPUT
CSTRESS,
*OUTPUT, HISTORY, OP=NEW
*ENERGY OUTPUT
ALLAE, ALLCD, ALLFD, ALLIE, ALLKE, ALLPD, ALLSE, ALLVD, ALLWK, ETOTAL
*NODE OUTPUT, NSET=BOTDIE
U, RF
*END STEP