** : symmetric transfer from base problem:smg_wedge_mismap-t1
*HEADING
** FEATURE TESTED : *SYMMETRIC MODEL GENERATION,PERIODIC
**                  *SYMMETRIC RESULTS TRANSFER
** ELEMENT TESTED : C3D8T
*preprint,model=yes,history=yes
*SYMMETRIC MODEL GENERATION,PERIODIC,ELEMENT=300,NODE=800
syma,symb
syma4,symb4
*SYMMETRIC RESULTS TRANSFER, STEP=1
*BOUNDARY
bot,1,3
padboun,1,1
padboun,2,2
left,1,2
right,1,2
*TRANSFORM,NSET=NALL,TYPE=C
*STEP,nlgeom
*coupled temperature-displacement,deltmx=10.0
0.1,1
*dload
pad,p2,100
*output,field,freq=999,var=preselect
*elset,elset=qa_test_print
print,
*output,field,freq=999
*node output,nset=qa_test_nset
nt,
**element output,elset=qa_test_print
**s,
*END STEP