*HEADING
 Transfer from Standard to Explicit : hyperelastic material
 - Explicit analysis
 [base for xs_s_cps3_hyper, references sx_s_cps3_hyper]
*IMPORT,UPDATE=NO,STATE=YES
ELALL,
*RESTART, WRITE
**
** step#1
**
**
*NSET, NSET=QA_TEST_ALLNODES
ALL,
**
*STEP
*DYNAMIC,EXPLICIT
,0.1
*BOUNDARY,TYPE=VELOCITY
FIX1,1,1
FIX2,2,2
DISP,1,,3.0
*FILE OUTPUT,TIMEMARKS=YES,NUM=1
*NODE FILE
U,
***OUTPUT,HISTORY,TIME INTERVAL=2.5E-3
***ELEMENT OUTPUT,ELSET=ELALL
**S,LE
*OUTPUT, FIELD, TIMEMARKS=YES, NUMBER INTERVAL=1
*NODE OUTPUT, NSET=QA_TEST_ALLNODES
U,
*OUTPUT,FIELD,VARIABLE=PRESELECT
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIMEINT=0.1
*ENDSTEP