*HEADING
*PREPRINT,MODEL=YES, ECHO=YES, HISTORY=YES
*IMPORT, UPDATE=NO,STATE=YES, STEP=1
SHELL1,SHELL2,SHELL3,SHELL4
*RESTART,WRITE
*NODE,NSET=NALL
*NSET,NSET=BOT
*NSET,NSET=LEFT
*NSET,NSET=RIGHT
*ELEMENT,TYPE=S4R,ELSET=SHELL101
*SHELL SECTION,ELSET=SHELL101, MATERIAL=SHELL1
1.0,
*REBAR LAYER, ORI=ORIENTS1
REBAR101,0.5,1.0,0,REBAR1,-15.0,1
**
*NODE,NSET=NALL
*NSET,NSET=BOT
*NSET,NSET=LEFT
*NSET,NSET=RIGHT
*ELEMENT,TYPE=S4R,ELSET=SHELL102
*SHELL SECTION,ELSET=SHELL102, MATERIAL=SHELL2
1.0,
*REBAR LAYER
REBAR102,0.5,1.0,0,REBAR2,0,1
**
*NODE,NSET=NALL
*NSET,NSET=BOT
*NSET,NSET=LEFT
*NSET,NSET=RIGHT
*ELEMENT,TYPE=S3R,ELSET=SHELL103
*SHELL SECTION,ELSET=SHELL103, MATERIAL=SHELL3
1.0,
*REBAR LAYER, ORI=ORIENTS3
REBAR103,0.5,1.0,0,REBAR3,-15.0,1
**
*NODE,NSET=NALL
*NSET,NSET=BOT
*NSET,NSET=LEFT
*NSET,NSET=RIGHT
*ELEMENT,TYPE=S3R,ELSET=SHELL104
*SHELL SECTION,ELSET=SHELL104, MATERIAL=SHELL4
1.0,
*REBAR LAYER
REBAR104,0.5,1.0,0,REBAR4,0,1
REBAR105,0.5,1.0,0,REBAR4,0,2
*ELSET,ELSET=EALL
SHELL1,SHELL2,SHELL3,SHELL4
SHELL101,SHELL102,SHELL103,SHELL104
*FILE FORMAT, ZERO INCREMENT
*STEP,NLGEOM, AMPLITUDE=RAMP
*STATIC
.2,1.
*BOUNDARY
NALL,3,6
LEFT, 1
BOT,  2
RIGHT,1,1,.075
*EL PRINT,ELSET=EALL,REBAR,FREQ=99
S,E,IVOL,RBFOR,RBANG,RBROT
*EL PRINT,ELSET=EALL
S,E
*EL FILE,ELSET=EALL, DIRECTION=YES
S
*EL FILE,ELSET=EALL, DIRECTION=YES
E
*EL FILE,ELSET=EALL,REBAR,FREQ=99
S,
*EL FILE,ELSET=EALL,REBAR,FREQ=99
IVOL,
*EL FILE,ELSET=EALL,REBAR,FREQ=99
RBFOR,
*EL FILE,ELSET=EALL,REBAR,FREQ=99
RBANG,
*EL FILE,ELSET=EALL,REBAR,FREQ=99
RBROT,
*NODE FILE, NSET=NALL
COORD,
*OUTPUT,FIELD,FREQ=99
*ELEMENT OUTPUT,ELSET=EALL,REBAR
S,E,IVOL,RBFOR,RBANG,RBROT
*ELEMENT OUTPUT,ELSET=EALL
S,E
*NODE OUTPUT
COORD,
*END STEP