*HEADING
 QUASI-STATIC TEST OF SHELL TO SOLID COUPLING
** JOB NAME: XSHELL2SOLID_S4R_C3D10M_XPL MODEL NAME: MODEL-1
*PREPRINT, MODEL=YES
**
** PARTS
**
*PART, NAME=PART-1
*END PART
*PART, NAME=PART-2
*END PART
**
** ASSEMBLY
**
*ASSEMBLY, NAME=ASSEMBLY
**
*INSTANCE, NAME=PART-1-1, PART=PART-1
*NODE, NSET=NALL
*ELEMENT, TYPE=C3D10M
** REGION: (SECTION-1:PICKED)
*ELSET, ELSET=_I1, INTERNAL, GENERATE
** SECTION: SECTION-1
*SOLID SECTION, ELSET=_I1, MATERIAL=MATERIAL-1,CONTROLS=CONT
1.,
*END INSTANCE
**
*INSTANCE, NAME=PART-2-1, PART=PART-2
*NODE, NSET=NALL
*ELEMENT, TYPE=S4R
** REGION: (SECTION-2:PICKED)
*ELSET, ELSET=_I1, INTERNAL, GENERATE
** SECTION: SECTION-2
*SHELL SECTION, ELSET=_I1, MATERIAL=MATERIAL-1, CONTROLS=CONT
0.25, 3
*END INSTANCE
*NSET, NSET=_G9, INTERNAL, INSTANCE=PART-1-1
*NSET, NSET=QA_TEST1, INSTANCE=PART-1-1
*ELSET, ELSET=_G9, INTERNAL, INSTANCE=PART-1-1
*NSET, NSET=_G10, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G11, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G12, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G13, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G14, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G15, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G16, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=_G17, INTERNAL, INSTANCE=PART-2-1
*NSET, NSET=QA_TEST2, INSTANCE=PART-2-1
*NSET, NSET=_G18, INTERNAL, INSTANCE=PART-1-1
*ELSET, ELSET=_G18, INTERNAL, INSTANCE=PART-1-1
*NSET, NSET=_G19, INTERNAL, INSTANCE=PART-1-1
*ELSET, ELSET=_G19, INTERNAL, INSTANCE=PART-1-1
*NSET, NSET=_G20, INTERNAL, INSTANCE=PART-2-1
*ELSET, ELSET=_G20, INTERNAL, INSTANCE=PART-2-1
*ELSET, ELSET=_SURF-1_S4, INTERNAL, INSTANCE=PART-1-1, GENERATE
*ELSET, ELSET=_SURF-1_S2, INTERNAL, INSTANCE=PART-1-1
*SURFACE, TYPE=ELEMENT, NAME=SURF-1
_SURF-1_S4, S4
_SURF-1_S2, S2
*ELSET, ELSET=_SURF-2_E4, INTERNAL, INSTANCE=PART-2-1
*ELSET, ELSET=_SURF-2_E2, INTERNAL, INSTANCE=PART-2-1
*SURFACE, TYPE=ELEMENT, NAME=SURF-2
_SURF-2_E4, E4
_SURF-2_E2, E2
** CONSTRAINT: CONSTRAINT-1
*SHELL TO SOLID COUPLING, CONSTRAINT NAME=CONSTRAINT-1,INFLUENCE DISTANCE=.125
SURF-2, SURF-1
*END ASSEMBLY
*SECTION CONTROLS, NAME=CONT, SECOND ORDER=YES
**
** MATERIALS
**
*MATERIAL, NAME=MATERIAL-1
*DENSITY
.5,
*ELASTIC
 3E+07, 0.3
*AMPLITUDE, NAME=AMP1,DEFINITION=SMOOTH STEP
0.0,0.0,1.,1.0
*AMPLITUDE, NAME=AMP2,DEFINITION=SMOOTH STEP
0.0,1.0,1.,0.0
*NSET, NSET=QA_TEST
ASSEMBLY.QA_TEST1, ASSEMBLY.QA_TEST2
** ----------------------------------------------------------------
**
** STEP: STEP-1
**
*STEP, NAME=STEP-1, NLGEOM=YES
BEND - NONLINEAR
*DYNAMIC, EXPLICIT
, 1.,
**
** BOUNDARY CONDITIONS
**
** NAME: BC-3 TYPE: DISPLACEMENT/ROTATION
*BOUNDARY
_G19, 1, 1
_G19, 2, 2
_G19, 3, 3
**
** LOADS
**
** NAME: LOAD-5   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP1
_G14, 2, -15.
** NAME: LOAD-6   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP1
_G15, 2, -30.
**
** OUTPUT REQUESTS
**
*RESTART, WRITE, NUMBER=1
**
** FIELD OUTPUT: F-OUTPUT-2
**
*OUTPUT, FIELD, N=2
*NODE OUTPUT, NSET=QA_TEST
U,
***ELEMENT OUTPUT
**S,
**
** HISTORY OUTPUT: H-OUTPUT-2
**
*OUTPUT, HISTORY, VARIABLE=PRESELECT
*END STEP
** ----------------------------------------------------------------
**
** STEP: STEP-2
**
*STEP, NAME=STEP-2, NLGEOM=YES
PULL - NONLINEAR
*DYNAMIC, EXPLICIT
, 1.,
**
** LOADS
**
** NAME: LOAD-7   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP1
_G16, 1, 15.
** NAME: LOAD-8   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP1
_G17, 1, 30.
*END STEP
** ----------------------------------------------------------------
**
** STEP: STEP-3
**
*STEP, NAME=STEP-3, NLGEOM=YES
UNLOAD
*DYNAMIC, EXPLICIT
, 1.,
**
** LOADS
**
** NAME: LOAD-5   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP2
_G14, 2, -15.
** NAME: LOAD-6   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP2
_G15, 2, -30.
** NAME: LOAD-7   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP2
_G16, 1, 15.
** NAME: LOAD-8   TYPE: CONCENTRATED FORCE
*CLOAD, AMPLITUDE=AMP2
_G17, 1, 30.
*END STEP
** ----------------------------------------------------------------
**
** STEP: STEP-4
**
*STEP, NAME=STEP-4, NLGEOM=YES
RIGID ROTATION
*DYNAMIC, EXPLICIT
, 1.,
**
** BOUNDARY CONDITIONS
**
** NAME: BC-3 TYPE: DISPLACEMENT/ROTATION
*BOUNDARY, OP=NEW
** NAME: BC-4 TYPE: DISPLACEMENT/ROTATION
*BOUNDARY, OP=NEW, AMPLITUDE=AMP1
_G20, 1, 1
_G20, 2, 2
_G20, 3, 3
_G20, 6, 6, -1.5708
*END STEP