*HEADING
ADAPTIVE MESHING EXAMPLE
FORGING WITH DUCK-SHAPED DIE (3D REVOLUTION)
Units - N, mm, sec
*NODE
**
**
*ELEMENT, TYPE=C3D8R, ELSET=BLANK
**
** xsymm
**
*NSET, NSET=XSYMM, GENERATE
**
** zsymm
**
*NSET, NSET=ZSYMM
**
*RESTART,WRITE,NUMBERINTERVAL=2
*NSET,NSET=REF
**
*MATERIAL,NAME=BLANK
*DENSITY
7340.e-9,
*ELASTIC
       2.E5,         0.3
*PLASTIC
      360.,          0.
      390.,          1.
*SOLID SECTION,ELSET=BLANK,MATERIAL=BLANK,CONTROLS=SECT
*SECTION CONTROLS,NAME=SECT,HOURGLASS=ENHANCED, KINEMATICS=ORTHOGONAL
*BOUNDARY
72001,1,6
72000,1,1
72000,3,6
XSYMM,1,1
ZSYMM,3,3
*ELSET,ELSET=OUT
*SURFACE,TYPE=ELEMENT,NAME=BLANK, REGION TYPE=SLIDING
BLANK,
*SURFACE, NAME=TOP, TYPE=REVOLUTION
START, .0, 25.229997
 LINE, 15.71, 24.949997
 LINE, 18.6371, 24.729697
 LINE, 21.55, 24.373797
 LINE, 24.4567, 23.976597
 LINE, 27.3761, 23.684397
 LINE, 29.9775, 22.409497
 LINE, 32.1287, 20.415797
 LINE, 33.832, 18.029097
 LINE, 34.6121, 15.211297
 LINE, 36.7348, 13.304597
 LINE, 39.6458, 13.019797
 LINE, 42.3904, 13.858497
 LINE, 44.2512, 16.115697
 LINE, 46.572499999, 17.824997
 LINE, 49.4593, 18.308497
 LINE, 52.38, 18.089997
 LINE, 76.19, 16.189997
 LINE, 78.7544, 15.803397
 LINE, 81.3444, 15.667597
 LINE, 83.935199999, 15.785597
 LINE, 86.4957, 16.193997
 LINE, 88.9693, 16.967397
 LINE, 91.2581, 18.179697
 LINE, 93.2268, 19.860797
 LINE, 94.809, 21.912997
 LINE, 96.0892, 24.168297
 LINE, 97.151099999, 26.534597
 LINE, 97.9595, 28.998497
 LINE, 98.4747, 31.540297
 LINE, 98.7994, 34.114297
 LINE, 99.1068, 36.690567
 LINE, 99.6008, 39.235957
 LINE, 100.532, 41.652007
 LINE, 101.927, 43.835926999
 LINE, 103.45, 45.933596
 LINE, 104.287, 44.366997
 LINE, 105.71, 42.275997
 LINE, 129.015, 42.275997
 LINE, 129.113, 42.279146999
 LINE, 129.21, 42.288637
 LINE, 129.306, 42.304356999
 LINE, 129.4, 42.326207
 LINE, 129.493, 42.354097
 LINE, 129.584, 42.387926999
 LINE, 129.672, 42.427597
 LINE, 129.758, 42.473006999
 LINE, 129.842, 42.524057
 LINE, 129.922, 42.581027
 LINE, 130.436, 42.971007
 LINE, 130.95, 43.360986999
 LINE, 131.464, 43.750957
 LINE, 131.978, 44.140937
 LINE, 132.058, 44.197927
 LINE, 132.142, 44.248977
 LINE, 132.227, 44.294387
 LINE, 132.316, 44.334057
 LINE, 132.407, 44.367886999
 LINE, 132.5, 44.395776999
 LINE, 132.594, 44.417637
 LINE, 132.69, 44.433346999
 LINE, 132.787, 44.442837
 LINE, 132.885, 44.445996999
 LINE, 163.8, 44.445996999
*SURFACE, NAME=BOT_1, TYPE=REVOLUTION
START,      150.47,       26.19
 LINE,     131.737,       26.19
 LINE,     131.644,     26.1856
 LINE,     131.552,     26.1727
 LINE,     131.462,     26.1514
 LINE,     131.374,     26.1218
 LINE,      131.29,     26.0843
 LINE,     131.209,     26.0389
 LINE,     131.132,     25.9859
 LINE,     130.796,     25.7305
 LINE,      130.46,      25.475
 LINE,     130.124,     25.2195
 LINE,     129.788,     24.9641
 LINE,     129.711,     24.9111
 LINE,      129.63,     24.8657
 LINE,     129.546,     24.8282
 LINE,     129.458,     24.7986
 LINE,     129.368,     24.7773
 LINE,     129.276,     24.7644
 LINE,     129.183,       24.76
 LINE,     105.486,       24.76
 LINE,     105.394,     24.7643
 LINE,     105.303,     24.7769
 LINE,     105.214,     24.7978
 LINE,     105.127,     24.8268
 LINE,     105.043,     24.8637
 LINE,     104.962,     24.9084
 LINE,     103.964,     25.7872
 LINE,     103.123,     26.8228
 LINE,     102.162,     27.7427
 LINE,      100.95,       28.28
 LINE,     100.849,       28.28
 LINE,     100.749,       28.28
 LINE,     100.648,       28.28
 LINE,     100.547,       28.28
 LINE,     100.447,       28.28
 LINE,     100.346,       28.28
 LINE,     100.245,       28.28
 LINE,     100.144,       28.28
 LINE,     100.044,       28.28
 LINE,     99.9431,       28.28
 LINE,     99.8424,       28.28
 LINE,     99.7417,       28.28
 LINE,      99.641,       28.28
 LINE,     99.5403,       28.28
 LINE,     99.4396,       28.28
 LINE,     99.3389,       28.28
 LINE,     99.2382,       28.28
 LINE,     99.1375,       28.28
 LINE,     99.0368,       28.28
 LINE,     98.9361,       28.28
 LINE,     98.8354,       28.28
 LINE,     98.7347,       28.28
 LINE,     98.6341,       28.28
 LINE,     98.5334,       28.28
 LINE,     98.4327,       28.28
 LINE,      98.332,       28.28
 LINE,     98.2313,       28.28
 LINE,     98.1306,       28.28
 LINE,     98.0299,       28.28
 LINE,     97.9292,       28.28
 LINE,     97.8285,       28.28
 LINE,     97.7278,       28.28
 LINE,     97.6271,       28.28
 LINE,     97.5264,       28.28
 LINE,     97.4257,       28.28
 LINE,     97.3251,       28.28
 LINE,     97.2243,       28.28
 LINE,     97.1237,       28.28
 LINE,      97.023,       28.28
 LINE,     96.9216,     28.2748
 LINE,     96.8224,     28.2597
 LINE,     96.7257,     28.2348
 LINE,      96.632,     28.2004
 LINE,     96.5421,     28.1568
 LINE,     96.4567,     28.1042
 LINE,      96.377,     28.0434
 LINE,     95.3397,     27.1116
 LINE,     94.3854,     26.0956
 LINE,     93.5723,     24.9645
 LINE,     92.9873,     23.7017
 LINE,     92.7309,     22.3353
 LINE,       92.85,       20.95
 LINE,     93.0208,     19.3061
 LINE,       93.04,     17.6538
 LINE,     92.9148,     16.0062
 LINE,     92.6523,     14.3747
 LINE,     92.2586,     12.7697
 LINE,      91.739,     11.2011
 LINE,     91.0975,     9.67813
 LINE,     90.3373,     8.21085
 LINE,     89.4609,     6.80994
 LINE,     88.4702,     5.48742
 LINE,     87.3672,     4.25701
 LINE,     86.1548,     3.13438
 LINE,     84.8375,      2.1371
 LINE,     83.4226,     1.28416
 LINE,     81.9213,    0.594672
 LINE,     80.3497,     0.08586
 LINE,     78.7282,   -0.229609
 LINE,     77.0803,   -0.346054
 LINE,     75.4303,   -0.266062
 LINE,        73.8,          0.
 LINE,        51.9,          2.
 LINE,     50.4463,     2.59858
 LINE,     49.0113,     3.24109
 LINE,     47.6137,     3.96153
 LINE,     46.3012,     4.82539
 LINE,     45.1472,     5.89009
 LINE,     44.1879,     7.13439
 LINE,     43.3386,     8.45763
 LINE,     42.4391,     9.74659
 LINE,     41.3527,     10.8793
 LINE,     40.0384,     11.7353
 LINE,     38.5394,     12.1834
 LINE,     37.0028,     11.9463
 LINE,     35.7417,     11.0272
 LINE,     34.8982,      9.7062
 LINE,     34.1557,     8.32105
 LINE,     33.2335,     7.04895
 LINE,     32.1781,      5.8841
 LINE,     31.0403,     4.79937
 LINE,     29.8367,     3.78811
 LINE,       28.57,       2.857
 LINE,     9.37914,    0.956866
 LINE,     9.28061,       0.952
 LINE,          0.,       0.952
*RIGID BODY,REF NODE=72000, ANALYTICAL SURFACE =BOT_1
*RIGID BODY,REF NODE=72001, ANALYTICAL SURFACE =TOP
*STEP
*DYNAMIC,EXPLICIT
,0.107
*VARIABLE MASS SCALING,DT=5.5E-6,TYPE=BELOW MIN,
ELSET=BLANK, FREQUENCY=10
*BOUNDARY,TYPE=VELOCITY
72000,2,2,-166.652
*CONTACT PAIR,INTERACTION=SMOOTH
BLANK,BOT_1
BLANK,TOP
*SURFACE INTERACTION,NAME=SMOOTH
*FILE OUTPUT,TIMEMARKS=YES,NUM=1
*EL FILE,ELSET=OUT
PEEQ,
*NODE FILE,NSET=REF
U,
***OUTPUT,HISTORY,TIME INTERVAL=1.0E-2
***NODE OUTPUT,NSET=REF
**RF1,RF2
***ENERGY OUTPUT
**ALLKE,ALLIE,ALLAE,ALLVD,ALLWK,ETOTAL,
**DT,
*ADAPTIVE MESH,ELSET=BLANK
*output,field,number=2
*element output
peeq,
*node output
u,
*****
*NSET, NSET=QA_TEST_REFN
REF,
*ELSET, ELSET=QA_TEST
OUT,
*NSET, NSET=QA_TEST
XSYMM,
*OUTPUT, FIELD, TIME MARKS=YES, NUMBER INTERVAL=1
*ELEMENT OUTPUT, ELSET=QA_TEST
PEEQ,
*NODE OUTPUT, NSET=QA_TEST
U,
*NODE OUTPUT, NSET=QA_TEST_REFN
RF,
*OUTPUT, HIST, FREQ=9999
*ENERGY OUTPUT, VAR=PRESELECT
******
*END STEP