*HEADING
 AXISYMMETRIC FORMING OF A CIRCULAR CUP: IMPORT OF RESULTS FROM ABQ/EXPLICIT
AFTER THE SECOND FORMING STEP FOR SPRINGBACK ANALYSIS
*IMPORT, STEP=2, INT=1, UPDATE=NO, STATE=YES
BLANK,
*BOUNDARY, FIXED
1, 1, 2
*RESTART, WRITE, FREQ=1
*ELSET, ELSET=QA_TEST, GEN
*ELSET, ELSET=QA_TEST
*NSET, NSET=QA_TEST, GEN
*STEP, NLGEOM, INC=50
*STATIC
1.E-04, 1.E-3
**************
*EL FILE, ELSET=QA_TEST, FREQ=999
STH,
*NODE FILE, NSET=QA_TEST, FREQ=999
U,
*OUTPUT,FIELD, FREQ =999
*ELEMENT OUTPUT, ELSET=QA_TEST
STH, PEEQ
*NODE OUTPUT, NSET=QA_TEST
U,
*OUTPUT,FIELD
*ELEMENT OUTPUT
STH,
*NODE OUTPUT
U,
*OUTPUT, HISTORY
*ENERGY OUTPUT, VAR=PRESELECT
**************
*END STEP