*HEADING
 Transfer from Standard to Explicit : MPCs sslinear and slider
 - Standard analysis
 [base for sx_x_c3d8r_mpcsslin, references xs_x_c3d8r_mpcsslin]
*RESTART,WRITE
*IMPORT,UPDATE=NO,STATE=YES
SOLID,SHELL
*ELSET,ELSET=ELALL
SOLID,SHELL
*MPC
SS LINEAR, 101,3,13,23
SS LINEAR, 111,6,16,26
SS LINEAR, 121,9,19,29
SLIDER, 13,3,23
SLIDER, 16,6,26
SLIDER, 19,9,29
**
** step#1
**
*STEP,NLGEOM
*STATIC
.1,1.
*BOUNDARY
CLAMPED,1,3
SYM,ZSYMM
EDGE,1,1,0.2
*NODE PRINT
 U,
 RF,
*NODE FILE
 U,
 RF,
*EL PRINT
 S,
 E,
*END STEP